*****************
 UNLOCKING ASUS R700/ASUS R300:
*****************
1. copy on the root of card this file:  ASUS_UserFlashCopy.dll
2. set switch to OFF, put the card in device then set switch to ON. device will boot-up in windows.
3. on the desktop device dubleclick on “USB loader”
4. select “Serial class” then “Activate”
5. connect device to PC and you have access to hidden partition from device with windows explore (you must have activsync installed).
enjoy!
NOTE: don’t forget to delete ASUS_UserFlashCopy.dll file from card when you finish


******************
UNLOCKING AND CHANGING DEFAULT NAVIGATION SOFTWARE
******************
1) * The default navigation software is Igo8 stored on the igo8 folder of the Sdcard *

      == OPTIONAL ==
   If you want the navigation button to run another software:
   Edit the file navigation.mscr with a text editor
   change the line that contains:     Run("\SDMMC\IGO8\igo8.exe")
   to whatever path/program you want.  
   
2) copy to the root of sdcard these files:
	ASUS_UserFlashCopy.dll
	MortScript.exe
	navigation.exe
	navigation.mscr

3) put the sdcard into the gps and switch power off and then on

4) once the gps booted up you will be on the WinCE desktop.  
   just tap on the my device icon (on the top left corner of the screen
   It will open up a file explorer window 

5) goto the \SDMMC folder and delete the file: ASUS_UserFlashCopy.dll

6) highlight the files:
	MortScript.exe
	navigation.exe
	navigation.mscr
   and select copy from the "edit" from the top menu bar

7) now goto the \FlashDisk\Navi folder
   select paste from the "edit" from the top menu bar
   when prompted to overwrite the files pick yes
  
  (if the task bar is covering the buttons, set the taskbar to autohide)

8) reboot the gps.

Now when you click on the navigation buttons it will run Igo8 from the SDCard or whatever program you set it to


***********************
For manual setup of navigation software, the port for the GPS chip is:
Port: 2
Baud: 57600  
+++++++++++++++++++++++++


